RME Intelligent Audio Solutions

Digiface AVB / Dante

MADIface Series Combo Driver Package for Windows 7/8/10 32/64

Includes MADIface series driver and MADIfaceNET driver for internal USB Ethernet adapter and AVB Controller

Important information: Driver version 0.9700 / 0.9442


Installation
-------------

Latest driver:
http://www.rme-audio.de/download/driver_madifacenet_win_xxxx.zip


Latest firmware
http://www.rme-audio.de/download/fut_ufxplus_avb_dante_win.zip


A firmware update is only possible if the driver had been installed before.

Follow the instructions of the RME Driver Install Wizard. This tool installs/updates all driver files. After that attach the device (in case of first time installation) or reboot (in case of an update) the computer.

----------------------

News, changes and fixes


V 0.9700 / 0.9442 (12/05/2019)

Please update to firmware version 210 !!!

- Improved MRP/SRP bandwidth reservation on sample rate change

- Changed core controller to run as Windows service. AVB now continues to work even when the AVB controller software is exit.

- Added extended stream configuration

- Added Presentation Time Offset per stream

- Added new Stream Format menu

- Fixes list corruption when multiple devices are switched off and on again

- Improved UI

- Deactivated cable detection (due to unreliable behavior)

- Fixed possible stop of receiving network data while transmitting continued

- AVB controller now compatible to Windows 8 (7). No longer uses QueryInterruptTime.

- A change in the Milan standard made Disconnect incompatible to the M32 Pro series - fixed

- Added AAF formats to the Inputs Format dialog

- New option to set the stream formats

- Bugfix in AVB endpoint for function SET_STREAM_FORMAT


--------------------

V 0.9685 / 0.9407 (08/01/2019)

- Added support for GET_NAME


--------------------

V 0.9685 / 0.9406 (06/25/2019)

- Added support for MIDI over MADI for MADI I/O of Digiface Dante. Requires firmware 36.

- Digiface AVB now supports 64 channels (instead of 60) at 192 kHz. Requires firmware 206.

- TotalMix FX version 1.61


--------------------

V 0.9684 / 0.9405 (05/06/2019)

- Bug fix Digiface Dante WDM recording: the WDM record devices 5/6 and 7/8 received the signal 5/6, all channels above 7/8 were shifted by 2 channels (v 0.9684)

- AVB: Quick discovery in Hive

- AVB: Removed some causes for error messages

- AVB: Made Configure dialog wider so no text cutting anymore

--------------------

V 0.9681 / 0.9402 (03/06/2019)

- AVB Controller improved: fixed device selection, added scrollable device list view. 


--------------------

V 0.9681 / 0.9400 (02/25/2019)

New in TotalMix FX 1.6:

- Settings for External Input and current PFL mode are no longer changed per Snapshot.

- Solo/PFL have now priority over the Mute state of an input channel.

- Settings, Mixer: New option 'Exclusive Solo/PFL Mode'

- Settings, Mixer: New option '2-Row Mode with only Input in first row'

- Settings, Aux Devices: Increased number of Aux device channel banks to 24, so that MADIface XT and HDSPe MADI FX can control an Octamic XTC even on MADI port 3.

- Preferences, Mixer Views: New option 'Store channel open/close state in Layout Preset'.

- Preferences, Snapshots: new 'do not load' options 'Main Volume, Main/Phones Volume, Control Room Settings'.

- Preferences, New Option 'Store Settings for all users'. So far every user had his own TM FX state/settings. This option now allows to have the same settings for all users.

-  Added full support for multi-user operation. On a user change TM FX will automatically close and reopen. According to the above option it then loads either specific settings for the current user, or the same settings for all users.

- Menu File: New option 'Preload all snapshots'. Loads the 8 snapshots of a workspace into the Snapshot section, but does not activate any of them. Other settings within the workspace file (window position etc.) are ignored.

- Matrix: Shift + click to change phase, Ctrl + click to mute (or double click) on the vertical channel name columns.   

- ARC USB: added new mode 'Push-or'. Allows for example to activate Talkback with a button and the footswitch without blocking each other.

- ARC USB, Usage: supports SysEx mode (requires firmware update of the ARC USB). Additional option to disable the former mode. Firmware download:

http://www.rme-audio.de/download/fut_arcusb_mac_v7.zip


Fixes:
- A locked user interface still allowed the double-click on a fader

- In rare situations the Mismatch message could cause a crash.

- Fixes different levels (0.05 dB) in level meters


----------------------

News, changes and fixes

V 0.9680 / 0.9400 (02/21/2019)

- The AVB controller now also stores all input stream formats of the m32 in xml format. Restoring the input streams works with ENTITY_DISCOVER without a timeout.


------------------------------

V 0.9680 / 0.9399 (02/19/2019)

- 'Set Stream Format' changed when changing the sample rate

- Requires firmware version 203 or higher


------------------------------

V 0.9680 / 0.9397 (01/11/2019)

- Full support for GET_AVB_INFO

- Requires firmware version 203 or higher


------------------------------

V 0.9680 / 0.9393 (11/21/2018)

- Bug fix: A Dante device could disturb the AVB network

- Added float format for macOS (full support upcoming) 

Completed support for Milan:

- Added Lock display for CRF

- Fixed word clock phase of CRF signal

- Setting the sample rate no longer changes the format (also valid for CRF/AAF)

- Reduced bandwidth for CRF streams

- Requires firmware version 202 or higher

------------------------------

V 0.9680 / 0.9391 (11/16/2018)

- Bug fix: PnP could cause wrong detection of a USB device and interrupt network streaming

First version to support Milan:

- Sending / receiving AAF in 44 / 88.2 / 176.4 / 192 kHz, 12 / 16 / 24 / 32 channel formats

- CRF (Clock Reference Format) with 0 channels (no audio)

- Requires firmware version 194 or higher


------------------------------

V 0.9680 / 0.9389 (11/05/2018)

- Minor improvement with storing WDM format

- Digiface Dante: Fixed the Settings dialog in USB2 mode


------------------------------


V 0.9673 (06/23/2018)

- WDM format restricted to 2-channel (stereo) and up to 7.1-channel (Multi-channel). Therefore the current setting stays even after reboot.

- Fix for Digiface USB WDM Phones Out at Double and Quad Speed

- Added support for Digiface AVB and Digiface Dante 

------------------------------



Copyright RME 12/2019
All rights reserved. Windows 7/8/10 are trademarks of Microsoft Corporation. ASIO is a trademark of Steinberg Media Technologies GmbH.

